The Final Format as used by the SASS-C IOSS and gengate add to one or  
more ASTERIX data blocks a 8 bytes header and a 4 bytes padding tail  
A5A5A5A5 in hex.  
The 8 bytes header is composed of:   
  
first two bytes: the message length in bytes;   
third to fifth byte: spares set to 0;   
sixth to eighth byte: the time of day since last midnight in 0.01  
second.